
[bookmark: _GoBack]附件2（会议墙报模板）：
（1）提交墙报要求：以PDF提交，0.8 m（宽）×1.8 m（长），清晰度300 ppi。
墙报样例：中文样例，英文样例（文末）。您也可以使用我们提供的墙报模板，更加便捷的制作您的墙报，形式内容不局限于此。
（2）会议报到当天与会务组联系领取墙报，自行张贴在同一展示区，会务组会为您提供必要的工具（胶带、图钉等）。
（3）论坛后会评选出“优秀墙报奖”，并颁发证书。
报名节点：请于2024年5月13日前将墙报+报名信息（可后期提交电子版，邮件请注明）发送至论坛官方邮箱zhengwen@iwt.cn，邮件主题为墙报展示+学校+姓名+联系方式（如：墙报展示-上海大学-王小二+13912345678），5月13日后未来得及提交的同学可自行打印墙报并携带至会场张贴（要求：画面尺寸宽80*高180㎝、PP纸、四角打孔，画面自带）。
（4）在墙报展示时段结束时，您还需要亲自取下您的墙报，请注意维护场地和设施的安全和整洁。
附墙报样本
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E-mail: shenyu@ectbu.edu.cn
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CaFeAl /LDQ
Agent for Wast

More than 35 million tons of wasted
mineral oil from industrial sector has
been produced globally annually. It
should be noted that heavy aromatics,
resins, asphaltenes, nitrogen-containing
heterocycle are main contaminants in
waste mineral oil Thus, without the
appropriate treatment. it has negative
impact on the environment.

Raw materials

Waste mineral oil was provided by Jihui
Remondis (Shanghaf) Environmental
Protection Technology Development Ltd.

Decolorizing agent preparation
LDH materials were prepared by co-
precipitation under low supersaturation
{eg. 50 mmol of Ca?*, 17 mmol of AR+ and
8 mmol of Fe** metal chlorate). The LDO
sample was calcined al 750 °C for 3 h

1o mesaporous saids

E-mail

- CaFeAlILDO decolorizing optimal condifions:
reaction at 60°C, reaction at 30min, dosage
5% and calcined at 750°C, the maximum
decolorization efficiency about 88%

- CaAIILDO decolorizing optimal conditions:
reaction at 50°C, reaction at 20min, dosage
6% and calcined at 750'C, the maximum
decolorization efficiency about 93%

- However the recycling rate of CaFeAllLDO is.
much higher than CaAULDO.





